# South Jordan Country Crossing Emergency Area

Net Script Sample

This is [name] [call sign], your Net Control Operator.

This is directed Net; all participating Stations please stand by. (Slight Pause)

Are there any stations with Emergency or Priority Traffic? If so, please come now.

(Listen for Emergency or Priority Traffic, if nothing is heard, say “Nothing Heard” and continue)

When your handle \ call sign is called, please speak 2-3 inches from the handheld slowly and clearly using your first name followed by your designation. Please include a signal quality report in addition to any traffic.

This is [*name][handle*], starting the roll call.

(designators might also be street and house number)

|  |
| --- |
| LOGAN10839 |
| LOGAN10848 |
| LOGAN10853 |
| SUMDAY10907 |
| SUMDAY10907 |
| SUMDAY10907 |
| SUMDAY10919 |
| MILLIE3247 |
| MILLIE3291 |
| MILLIE3291 |
| MILLIE3307 |
| MILLIE3307 |
| MILLIE3321 |
| MILLIE3333 |
| MILLIE3353 |
| MILLIE3366 |
| WESTSPRING3258 |
| WESTSPRING3271 |
| WESTSPRING3280 |
| WESTSPRING3290 |
| WESTSPRING3306 |
| WESTSPRING3306 |
| WESTSPRING3307 |
| WESTSPRING3325 |
| WESTSPRING3336 |
| WESTSPRING3336 |
| WESTSPRING3336 |
| WESTSPRING3343 |
| WESTSPRING3379 |

(Once you have read the names of all participating stations, say)

**“Are there any late or missed stations that would like to check in? If so, please come now.”**

(Pause for late or missing member check-ins; if nothing is heard, say “**Nothing Heard**” and continue)

To comment, wait for a pause and say “comment” followed by [name or *call sign*].

To break, say “break” “break” followed by [name or *call sign*].

To ask questions, wait for a pause and say “question” followed by [name or *call sign*].

Always wait for the Net control to say “Go ahead [name or *call sign*].

Provide any training or Information.

Are there any other announcements?

(Pause for announcements; if nothing is heard, say “**Nothing Heard**” and continue)

(When you are ready to close the Safety Net)

Thank you for your participation in today’s Net. I now return this channel to normal operation. This is [name][handle] 73 to all out and clear.